Standard Operating Procedure

Nitric Acid

*This is an SOP template and is not complete until: 1) lab specific information is entered into the box below 2) lab specific protocol/procedure is added to the protocol/procedure section and   
3) SOP has been signed and dated by the PI and relevant lab personnel.*

Print a copy and insert into your   
*Laboratory Safety Manual* and *Chemical Hygiene Plan*.   
Refer to instructions for assistance.

|  |  |
| --- | --- |
| **Department:** | Chemistry |
| **Date SOP was written:** | 11/26/2012 |
| **Date SOP was approved by PI/lab supervisor:** | 11/27/2102 |
| **Principal Investigator:** | Richmond Sarpong |
| **Internal Lab Safety Coordinator/Lab Manager:** | Rebecca Murphy |
| **Lab Phone:** | 510-643-2485 |
| **Office Phone:** | 510-643-6312 |
| **Emergency Contact:** | Richmond Sarpong 626-644-2407 |
| *(Name and Phone Number)* |
| **Location(s) covered by this SOP:** | Latimer 834, 836, 837, 838, 842, 844, 847, 849, 907 |
| *(Building/Room Number)* |

**Type of SOP:** ☐ Process ☒Hazardous Chemical ☐ Hazardous Class

**Purpose**

Nitric acid (also known as aqua fortis) is an extremely corrosive acid and strong oxidizing agent. It may be harmful if ingested, inhaled, or absorbed through the skin. It can cause severe skin and eye burns resulting in irreversible damage. It is extremely destructive to the tissue of the mucous membranes and the upper respiratory tract. The main use of nitric acid is in the production of agricultural fertilizers. Its other uses include the production of nylon precursors, explosives, and rocket fuel.

**Physical & Chemical Properties/Definition of Chemical Group**

CAS#: 7697-37-2

Class: **Corrosive, strong acids**

Molecular Formula: HNO3

Form (physical state): Liquid

Color: Colorless, light yellow

Boiling point: 83.9-100 °C

**Potential Hazards/Toxicity**

Nitric acid is an oxidizer that may intensify fires. Fire conditions may cause formation of hazardous nitrogen oxides. Nitric acid may be harmful if inhaled, ingested, or absorbed through the skin. It is extremely destructive to the tissue of the mucous membranes and upper respiratory tract. Causes severe skin and eye burns. May cause blindness and permanent eye damage. Inhalation may cause spasms, inflammation and edema of the bronchi or larynx, and pneumonitis. Other symptoms include burning sensation, coughing, wheezing, laryngitis, shortness of breath, headache, nausea, vomiting, and pulmonary edema. Effects may be delayed. Large doses may cause conversion of hemoglobin to methemoglobin, producing cyanosis or a drastic fall in blood pressure, leading to collapse, coma, and possibly death. Chronic exposure may cause erosion of the teeth, jaw necrosis, and kidney damage.

**Engineering Controls**

NOTE: Lab-specific information on engineering controls may be included in the Protocol/Procedure section.

Work with concentrated nitric acid should be conducted in a fume hood unless other controls are designated in the Protocol/Procedure section. Sash height should be kept low to minimize escaping fumes and provide a physical barrier.

**Personal Protective Equipment (PPE)**

NOTE: Lab-specific information on PPE selection may be included in the Protocol/Procedure section.

**Respirator Protection**

NOTE: Lab personnel intending to use/wear a respirator mask must be trained and fit-tested by EH&S. This is a regulatory requirement.

Refer to 8 CCR 5144 for selection of respirators. A respiratory protection program that meets 8 CCR 5144 must be followed whenever workplace conditions warrant use of a respirator.

Respirators should be used only under any of the following circumstances:

* As a last line of defense (i.e., after engineering and administrative controls have been exhausted).
* When Permissible Exposure Limit (PEL) has exceeded or when there is a possibility that PEL will be exceeded, and the material has adequate warning properties (e.g., odor or taste).
* Regulations require the use of a respirator.
* An employer requires the use of a respirator.
* There is potential for harmful exposure due to an atmospheric contaminant (in the absence of PEL)
* As PPE in the event of a chemical spill clean-up process

Lab personnel intending to use/wear a respirator mask must be trained and fit-tested by EH&S. This is a regulatory requirement.

**Hand Protection**

Handle with gloves. Viton gloves are recommended. Nitrile gloves are not recommended for concentrated (>70%) nitric acid according to the Ansell Chemical Resistance Guide. Gloves must be inspected prior to use. Use proper glove-removal technique (without touching glove’s outer surface) to avoid skin contact with this material. Wash and dry hands.

NOTE: Consult with your preferred glove manufacturer to ensure that the gloves you plan on using are compatible with nitric acid. Lab-specific information on glove selection may be included in the Protocol/Procedure section.

For glove selection, go to: <http://ehs.berkeley.edu/hs/63-laboratory-safety/94-glove-selection-and-usage.html>

Refer to glove selection chart from the links below:

<http://www.ansellpro.com/download/Ansell_8thEditionChemicalResistanceGuide.pdf>

OR

<http://www.allsafetyproducts.biz/page/74172>

OR

<http://www.showabestglove.com/site/default.aspx>

OR

<http://www.mapaglove.com/>

**Eye Protection**

Use safety glasses with side shields or tightly fitting safety goggles. Use face shield (8-inch minimum) over goggles when appropriate. Use equipment for eye protection tested and approved under appropriate government standards such as ANSI Z87.1, NIOSH (US), or EN 166(EU).

**Skin and Body Protection**

Long pants, closed-toed and closed-heeled shoes, cotton-based clothing/attire (no skin exposed below waist), and a *flame resistant lab coat* must be worn for protecting against chemical hazards. Use of a safety apron is also recommended for additional protection.

**Hygiene Measures**

Avoid contact with skin, eyes and clothing. Wash hands before breaks and immediately after handling the product.

**First Aid Procedures**

Notify supervisor and EH&S immediately following completion of first aid procedures. Follow up with a call to 510-642-9090 to report the incident.

**If inhaled**

Move person into fresh air. If not breathing, give artificial respiration. Call 911. Consult a physician.

**In case of skin contact**

Wash off with soap and plenty of water for at least 15 minutes and remove contaminated clothing. Consult a physician.

**In case of eye contact**

Rinse thoroughly with plenty of water for at least 15 minutes lifting upper and lower eyelids and removing contact lenses. Consult a physician. Continue rinsing eyes during transport to hospital.

**If swallowed**

Do not induce vomiting. Never give anything by mouth to an unconscious person. Rinse mouth with water. Consult a physician.

**Special Handling and Storage Requirements**

NOTE: Lab-specific information on handling and storage may be included in the Protocol/Procedure section.

**Working alone** Certain extremely hazardous operations should not be performed if the PI or Lab Safety Contact(s) are not present. Never work alone with extremely hazardous materials/operations. See the Protocol/Procedure section below for specific prohibitions (if any) on working alone.

**Precautions for safe handling:** Avoid contact with skin, eyes, and clothing. Avoid inhalation and ingestion. Keep away from heat and sources of ignition- No smoking.

**Conditions for safe storage:** Keep container tightly closed in a dry and well-ventilated area. Store in original container away from direct sunlight. Opened containers must be carefully resealed and stored upright to prevent leakage. Store away from combustible materials. Avoid alkali metals, reducing agents, cyanides, aldehydes, powdered metals organic materials, ammonia, acetic anhydride, acetonitrile, alcohols, and acrylonitrile.

**Spill and Accident Procedure**

**Chemical Spill - Dial 911**

**Spill** – Assess the extent of danger. Help contaminated or injured persons. Evacuate the spill area. Avoid breathing vapors. If possible, confine the spill to a small area using a spill kit or absorbent material. Keep others from entering contaminated area (e.g., use caution tape, barriers, etc.).

**Small ( < 1 L)** – If you have training, you may assist in the clean-up effort. Use appropriate personal protective equipment and clean-up material for chemical spilled. Double bag spill waste in clear plastic bags, label and take to the next chemical waste pick-up.

**Large (>1 L)** – Dial **911** and 510-642-9090 for assistance.

**Chemical Spill on Body or Clothes** – Remove clothing and rinse body thoroughly in emergency shower for at least 15 minutes. Seek medical attention. *Notify supervisor and EH&S immediately.* Follow up with a call to 510-642-9090 to report the incident.

**Chemical Splash Into Eyes** – Immediately rinse eyeball and inner surface of eyelid with water from the emergency eyewash station for 15 minutes by forcibly holding the eye open. Seek medical attention. *Notify supervisor and EH&S immediately.* Follow up with a call to 510-642-9090 to report the incident.

# **Medical Emergency Dial 911**

**Life Threatening Emergency, After Hours, Weekends And Holidays** – Dial **911** or go to the nearest emergency room. Note: All serious injuries must be reported to EH&S within 8 hours. Follow up with a call to 510-642-9090 to report the incident.

**Non-Life Threatening Emergency** – Go to the Occupational Health Facility (Tang Health Center). After hours go to the nearest emergency room. *Note: All serious injuries must be reported to EH&S within 8 hours. Follow up with a call to 510-642-9090 to report the incident.*

**Needle stick/puncture** **exposure** (as applicable to chemical handling procedure) – Wash the affected area with antiseptic soap and warm water for 15 minutes. For mucous membrane exposure, flush the affected area for 15 minutes using an eyewash station. Go to the Occupational Health Facility (Tang Health Center). After hours, go to the nearest emergency room. *Note: All needle stick/puncture exposures must be reported to EH&S within 8 hours. Follow up with a call to 510-642-9090 to report the incident.*

**Decontamination/Waste Disposal Procedure**

NOTE: Lab-specific information on decontamination/waste disposal may be included in the Protocol/Procedure section.

Wearing proper PPE, decontaminate equipment and bench tops using soap and water. Dispose of the used chemical and contaminated disposables as hazardous waste following the guidelines below.

*General hazardous waste disposal guidelines:*

**Label Waste**

Label all containers with the label provided at <http://ehs.berkeley.edu/hm/279-new-hazardous-waste-program-hwp.html>. See the EH&S Fact Sheet, “[Hazardous Waste Management”](http://ehs.berkeley.edu/images/ehs/pubs/52hazwaste.pdf) for general instructions on procedures for disposing of hazardous waste.

**Dispose of Waste**

* Dispose of regularly generated chemical waste within 90 days
* Call EH&S with questions

**Safety Data Sheet (SDS) Location**

SDS can be accessed online at <http://ucmsds.com>.

**Protocol/Procedure**

Nitric acid is a reagent used in organic reactions, and is a strong, corrosive acid and oxidizing agent.

Researchers should wear flame resistant lab coats, gloves, and safety goggles or glasses when handling nitric acid.

All work with concentrated nitric acid should be done inside a fume hood.

As a reagent, nitric acid may be used in quantities of <1mL up to 1L, and across a wide range of temperatures.

When working with concentrated nitric acid, it is important to make sure the work area is free of any bases and these may react violently with the acid.

It is also common to prepare dilute solutions of nitric acid for use as reagents, or for working up organic reactions.

When diluting nitric acid with water, the concentrated nitric acid should be added slowly to cooled water to minimize the exothermic nature of the reaction and any dangers from splashing.

Any solutions which contain nitric acid should be disposed of as hazardous waste after reactions are complete.

Nitric acid should be stored in a secondary container inside a designated corrosive cabinet.

Nitric acid should be stored in a separate area from any bases due to the danger of an exothermic reaction if allowed to mix.

As an oxidizing agent, nitric acid should be kept separate from organics that are flammable.

**NOTE**

Any deviation from this SOP requires approval from PI.

**Documentation of Training** (signature of all users is required)

* Prior to conducting any work with nitric acid, designated personnel must provide training to his/her laboratory personnel specific to the hazards involved in working with this substance, work area decontamination, and emergency procedures.
* The Principal Investigator must provide his/her laboratory personnel with a copy of this SOP and a copy of the SDS provided by the manufacturer.
* The Principal Investigator must ensure that their laboratory personnel have completed appropriate laboratory safety training and are current with any refresher training required.

I have read and understand the content of this SOP:

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Signature** | **Identification** | **Date** |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |
| Click here to enter text. |  |  | Click here to enter a date. |